Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| JavaTM 2 Platform Std. Ed. v1.4.2
PREV NEXT | FRAMES NO FRAMES

## Uses of Class
javax.print.attribute.standard.PrinterStateReason

Packages that use PrinterStateReason
javax.print.attribute.standard | Package javax.print.attribute.standard contains classes for specific printing attributes.

Uses of PrinterStateReason in javax.print.attribute.standard

Fields in javax.print.attribute.standard declared as PrinterStateReason
`static PrinterStateReason` | `PrinterStateReason.OTHER` The printer has detected an error other than ones listed below.
`static PrinterStateReason` | `PrinterStateReason.MEDIA_NEEDED` A tray has run out of media.
`static PrinterStateReason` | `PrinterStateReason.MEDIA_JAM` The device has a media jam.
`static PrinterStateReason` | `PrinterStateReason.MOVING_TO_PAUSED` Someone has paused the printer, but the device(s) are taking an appreciable time to stop.
`static PrinterStateReason` | `PrinterStateReason.PAUSED` Someone has paused the printer and the printer's `PrinterState` is STOPPED.
`static PrinterStateReason` | `PrinterStateReason.SHUTDOWN` Someone has removed a printer from service, and the device may be powered down or physically removed.
`static PrinterStateReason` | `PrinterStateReason.CONNECTING_TO_DEVICE` The printer has scheduled a job on the output device and is in the process of connecting to a shared network output device (and might not be able to actually start printing the job for an arbitrarily long time depending on the usage of the output device by other servers on the network).
`static PrinterStateReason` | `PrinterStateReason.TIMED_OUT` The server was able to connect to the output device (or is always connected), but was unable to get a response from the output device.
`static PrinterStateReason` | `PrinterStateReason.STOPPING` The printer is in the process of stopping the device and will be stopped in a while.
`static PrinterStateReason` | `PrinterStateReason.STOPPED_PARTLY` When a printer controls more than one output device, this reason indicates that one or more output devices are stopped.
`static PrinterStateReason` | `PrinterStateReason.TONER_LOW` The device is low on toner.
`static PrinterStateReason` | `PrinterStateReason.TONER_EMPTY` The device is out of toner.
`static PrinterStateReason` | `PrinterStateReason.SPOOL_AREA_FULL` The limit of persistent storage allocated for spooling has been reached.
`static PrinterStateReason` | `PrinterStateReason.COVER_OPEN` One or more covers on the device are open.
`static PrinterStateReason` | `PrinterStateReason.INTERLOCK_OPEN` One or more interlock devices on the printer are unlocked.
`static PrinterStateReason` | `PrinterStateReason.DOOR_OPEN` One or more doors on the device are open.
`static PrinterStateReason` | `PrinterStateReason.INPUT_TRAY_MISSING` One or more input trays are not in the device.
`static PrinterStateReason` | `PrinterStateReason.MEDIA_LOW` At least one input tray is low on media.
`static PrinterStateReason` | `PrinterStateReason.MEDIA_EMPTY` At least one input tray is empty.
`static PrinterStateReason` | `PrinterStateReason.OUTPUT_TRAY_MISSING` One or more output trays are not in the device.
`static PrinterStateReason` | `PrinterStateReason.OUTPUT_AREA_ALMOST_FULL` One or more output areas are almost full (e.g.
`static PrinterStateReason` | `PrinterStateReason.OUTPUT_AREA_FULL` One or more output areas are full (e.g.
`static PrinterStateReason` | `PrinterStateReason.MARKER_SUPPLY_LOW` The device is low on at least one marker supply (e.g.
`static PrinterStateReason` | `PrinterStateReason.MARKER_SUPPLY_EMPTY` The device is out of at least one marker supply (e.g.
`static PrinterStateReason` | `PrinterStateReason.MARKER_WASTE_ALMOST_FULL` The device marker supply waste receptacle is almost full.
`static PrinterStateReason` | `PrinterStateReason.MARKER_WASTE_FULL` The device marker supply waste receptacle is full.
`static PrinterStateReason` | `PrinterStateReason.FUSER_OVER_TEMP` The fuser temperature is above normal.
`static PrinterStateReason` | `PrinterStateReason.FUSER_UNDER_TEMP` The fuser temperature is below normal.
`static PrinterStateReason` | `PrinterStateReason.OPC_NEAR_EOL` The optical photo conductor is near end of life.
`static PrinterStateReason` | `PrinterStateReason.OPC_LIFE_OVER` The optical photo conductor is no longer functioning.
`static PrinterStateReason` | `PrinterStateReason.DEVELOPER_LOW` The device is low on developer.
`static PrinterStateReason` | `PrinterStateReason.DEVELOPER_EMPTY` The device is out of developer.
`static PrinterStateReason` | `PrinterStateReason.INTERPRETER_RESOURCE_UNAVAILABLE` An interpreter resource is unavailable (e.g., font, form).

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| JavaTM 2 Platform Std. Ed. v1.4.2
PREV NEXT | FRAMES NO FRAMES

Submit a bug or feature
For further API reference and developer documentation, see Java 2 SDK SE Developer Documentation. That documentation contains more detailed, developer-targeted descriptions, with conceptual overviews, definitions of terms, workarounds, and working code examples.

Copyright 2003 Sun Microsystems, Inc. All rights reserved. Use is subject to license terms. Also see the documentation redistribution policy.